**Instruction for LED name badge**

1. Put the CD into Computer CDROM. (Or get program file from our email)

2. Run the file “install.exe”

3. Select one of “Easy/ Professional/Help”

4. There will be 2 icons on Desktop:

1) Mini LED Display—Easy Program

It supports Chinese/ English / Korean / Japanese. Message Font and Size is Automatic

2) BMP Badge—Professional Program

It supports Global Language Editing. (Software support Chinese/English /Korean /Japanese)

Users can manually edit Message Font, Size, Image, Animation, etc.

5. Run the Easy Program (Mini LED Display)

Settings—Language—Select English/Spanish/Japanese/Korean/Chinese

Settings—Options—Tick 11 for Model# S1144, B1144, GD1144, LG1144, S1155

Tick 12 for Model# S1248, B1248, GD1248,

6. Use USB Connect Badge to Computer.

Drop-down left bottom “Port” window—Select “USB0” (Usually it automatically USB0)


7. Edit and Send Message

Input 1-8 messages as per your demand

Select display Speed — Level 1 Lowest to Level 8 Fastest)

Select display Effect — Freeze, Scroll, Laser, Snow, Animation, etc.

Select the message you want to display, click “Send”




8. LED Badge display the message

M1-8 is Circular display all selected messages

Press Message Key is fixed display current message.

9. If need more function, use Professional Program to manually edit message.

10. Function Keys—S1144, B1144, S1248, B1248



11. Function Keys— GD1144, GD1248, GD1133

